Overview | Package | Class | Source | Class tree | Glossary | UnrealScript Documentation
previous class next class | frames no frames

# IpDrv.UdpLink

00001 00002 00003 00004 00005
00006
00007
00008
00009
00010
00011
00012
00013
00014
00015
00016
00017
00018
00019
00020
00021
00022
00023
00024
00025
00026
00027
00028
00029
00030
00031
00032
00033
00034
00035
00036
00037
00038
00039
00040
00041
00042
00043
00044
00045
00046
00047
00048
00049
00050
00051
00052
00053
00054
00055
00056
00057
00058

    //=============================================================================
    // UdpLink: An Internet UDP connectionless socket.
    //=============================================================================
    class UdpLink extends InternetLink
    	native
    	transient;

    cpptext
    {
    	AUdpLink();
    	void PostScriptDestroyed();
    	UBOOL Tick( FLOAT DeltaTime, enum ELevelTick TickType );
    	FSocketData GetSocketData();
    }

    //-----------------------------------------------------------------------------
    // Variables.

    var() const int BroadcastAddr;

    //-----------------------------------------------------------------------------
    // Natives.

    // BindPort: Binds a free port or optional port specified in argument one.
    native function int BindPort( optional int Port, optional bool bUseNextAvailable );

    // SendText: Sends text string.
    // Appends a cr/lf if LinkMode=MODE_Line .
    native function bool SendText( IpAddr Addr, coerce string Str );

    // SendBinary: Send data as a byte array.
    native function bool SendBinary( IpAddr Addr, int Count, byte B[255] );

    // ReadText: Reads text string.
    // Returns number of bytes read.
    native function int ReadText( out IpAddr Addr, out string Str );

    // ReadBinary: Read data as a byte array.
    native function int ReadBinary( out IpAddr Addr, int Count, out byte B[255] );

    //-----------------------------------------------------------------------------
    // Events.

    // ReceivedText: Called when data is received and connection mode is MODE_Text.
    event ReceivedText( IpAddr Addr, string Text );

    // ReceivedLine: Called when data is received and connection mode is MODE_Line.
    event ReceivedLine( IpAddr Addr, string Line );

    // ReceivedBinary: Called when data is received and connection mode is MODE_Binary.
    event ReceivedBinary( IpAddr Addr, int Count, byte B[255] );

    defaultproperties
    {
         bAlwaysTick=True
    	 BroadcastAddr=-1;
    }

Overview | Package | Class | Source | Class tree | Glossary | UnrealScript Documentation
previous class next class | frames no frames

Class file time: ne 5.9.2004 16:02:16.000 - Creation time: st 23.5.2018 00:10:49.775 - Created with UnCodeX